**Patient Care Equipment Testing and Inspection Form**

|  |
| --- |
| **Per the NFPA 99, 2012 edition, Chapter 10, providers must test and visually inspect patient care equipment upon placing the device into service for the first time, whenever the device is repaired or modified, and additional frequencies as determined appropriate. Refer to the Patient Care Equipment Testing and Inspection Policy and Procedures for specific guidance on testing.**  |
| **Date** | **Electrical Patient Care Device** | **Reason for Testing** | **Visual Inspection** | **Testing** | **Completed by** |
| **Power Cord** | **Attachment Plug** | **Cord-Strain Relief** | **Continuity** | **Polarity** | **Resistance Testing** | **Leakage Testing** |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |